% tunet und eduroam down...

\section{Rep:1.a}
Own IP: 192.168.67.37

\section{Rep:1.b}
192.168.67.83

\section{Rep:1.c}
ip.addr == 192.168.67.83

\section{Rep:1.d}
Unusable features:
No. -> generated while monitoring
fixed values:
Source (192.168.67.83), Destination (192.168.67.37), Protocol (UDP), Length (82), TTL (64), Dest port (118), Flags (empty), Frag offset (0)


\section{Rep:1.e}


repeating transfers, transfers seem separable over time via the udp.srcport attribute

filtered traffic via wireshark again by source port 51899

reexported to csv

reimported to rapidminer

\section{Rep:1.f}
dscp + timing changes.

the DSCP value grows until 10962
grows until time 6.55
then it's fixed on DSCP 10962

\section{Rep:1.g}
Dest port == 118

\section{Rep:1.h}
siehe bladecode.py

\section{Rep:1.i}
some bits are broken, as the timing and my decodes is more a hack.

a hack is a hack is a hack ... :)























